[15] INTAKE AND EXHAUST - - AIR CLEANER - REMOVAL AND INSTALLATION <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G69>
CAUTION Parts marked by * are made of recycled-paper mixed plastic material, so observe the following precautions. Avoid any shock or load to these parts when removing and installing them. When installing, securely set the air cleaner cover and the resonator clamp to the air cleaner body. NOTE: Parts marked by * are made of recycled-paper mixed plastic material. Dispose of according to state and local laws
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Resonator
|  | 2. | Air cleaner element
|  | 3. | Air duct
|  | 4. | Air cleaner body
|  | 5. | Air flow sensor connector
|  | 6. | Breather hose connection
|  | 7. | Air flow sensor assembly
|  | 8. | Air cleaner cover
|  | 9. | Resonator
|  | 10. | Air intake hose
|  | 11. | Air cleaner bracket

[15] INTAKE AND EXHAUST - - AIR CLEANER - REMOVAL AND INSTALLATION <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation