[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - VACUUM HOSE - VACUUM HOSE PIPING DIAGRAM | PRINT PAGE / INDEX / PRIOR / NEXT

VACUUM HOSE

VACUUM HOSE PIPING DIAGRAM <4G63-SOHC> <4G63-DOHC> <4G64> <4G69 Vehicles except for Brazil, Chile and Hong kong> <4G69 Vehicles for Brazil and Chile> NOTE: The evaporative emission ventilation solenoid valve [always OPEN (OFF)], fuel tank differential pressure sensor, fuel level gauge, fuel temperature sensor are not used for engine control. <4G69 Vehicles for Hong kong>

[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - VACUUM HOSE - VACUUM HOSE PIPING DIAGRAM | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation