[55A] HEATER, AIR CONDITIONER AND VENTILATION - - TROUBLESHOOTING - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 6: The A/C Indicator Flashes. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 6: The A/C Indicator Flashes.
COMMENTS ON TROUBLE SYMPTOM If the A/C indicator flashes then the possible causes may be due to a defective A/C pressure system or insufficient refrigerant gas.
TROUBLESHOOTING HINTS Malfunction of the A/C pressure sensor Malfunction of the air thermo sensor Malfunction of the manual air conditioner control panel (A/C-ECU)
| DIAGNOSIS
| Step 1. Check the A/C pressure sensor operation. Refer to . Q: Is the check result normal? YES: Go to Step 2. NO: Replace the A/C pressure sensor.
| Step 2. Check the air thermo sensor. Refer to . Q: Is the check result normal? YES: Go to Step 3. NO: Replace the air thermo sensor.
| Step 3. Check the refrigerant level. Refer to . Q: Is the check result normal? YES: Replace the manual air conditioner control panel (A/C-ECU). NO: Correct the refrigerant level (Refer to ).

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - TROUBLESHOOTING - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 6: The A/C Indicator Flashes. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation