[25] PROPELLER SHAFT - - PROPELLER SHAFT - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| Check the sleeve yoke and centre yoke for wear, damage or cracks. Check the propeller shaft for bends, twisting or damage. Check the universal joint for smooth operation in all directions. Check the centre bearing for smooth movement.
| PROPELLER SHAFT RUNOUT
| Limit: 0.6 mm

[25] PROPELLER SHAFT - - PROPELLER SHAFT - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation