[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - OUTPUT SHAFT - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

OUTPUT SHAFT

DISASSEMBLY AND REASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
<<A>> | >>C<< | 1. | Transfer driven gear
|  | 2. | Bearing retainer
| >>B<< | 3. | Outer race
<<B>> | >>A<< | 4. | Taper roller bearing
|  | 5. | Output shaft
| DISASSEMBLY SERVICE POINTS
| <<A>> TRANSFER DRIVEN GEAR REMOVAL
| Use the special tool Bearing remover (MD998917) to remove the transfer driven gear.
| <<B>> TAPER ROLLER BEARING REMOVAL
| Use the special tool Bearing remover (MD998801) to remove the taper roller bearing.
| REASSEMBLY SERVICE POINTS
| >>A<< TAPER ROLLER BEARING INSTALLATION
| Use the special tools to install the taper roller bearing. Installer cap (MD998812) Installer 200 (MD998814) Installer adapter (MD998823)
| >>B<< OUTER RACE INSTALLATION
| Use the special tools to install the outer race. Installer adapter (MB990936) Handle (MB990938)
| >>C<< TRANSFER DRIVEN GEAR INSTALLATION
| Use the special tools to install the transfer driven gear. Installer cap (MD998812) Installer 100 (MD998813) Installer adapter (MD998823)

[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - OUTPUT SHAFT - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation