[1] PRE-DELIVERY INSPECTION - - UNDER HOOD - 10. BATTERY CONDITION AND CONNECTIONS | PRINT PAGE / INDEX / PRIOR / NEXT

| 10. BATTERY CONDITION AND CONNECTIONS
| Inspect the battery connections. Verify that they are tightened. NOTE: Do not wipe the lubricant from the battery posts and cable clamps.

[1] PRE-DELIVERY INSPECTION - - UNDER HOOD - 10. BATTERY CONDITION AND CONNECTIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation