[55A] HEATER, AIR CONDITIONER AND VENTILATION - - EVAPORATOR ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| AIR THERMO SENSOR INSPECTION
| INLET SIDE Measure the resistance between connector terminals 1 and 3 under at least two different temperatures. The resistance values should generally match those in the graph. NOTE: The temperature at the check should not exceed the range in the graph.
| OUTLET SIDE Measure the resistance between connector terminals 4 and 5 under at least two different temperatures. The resistance values should generally match those in the graph. NOTE: The temperature at the check should not exceed the range in the graph.

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - EVAPORATOR ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation