[1] PRE-DELIVERY INSPECTION - - UNDER VEHICLE - 14. SUSPENSION SYSTEM | PRINT PAGE / INDEX / PRIOR / NEXT

| 14. SUSPENSION SYSTEM
| Check to be sure that each installation bolt and nut is tightened. If split pins are used, make sure that they are properly installed. Lower arm, Upper arm Stabilizer bar Strut assembly
| REMOVE FRONT SPRING RESTRAINTS
| With the vehicle correctly positioned on the sub-frame contact points, and the suspension fully extended, remove the rubber restraints from the front springs. CAUTION It is very important that these restraints must be removed during predelivery-inspection. Failure to do so could cause ride and handling complaints.

[1] PRE-DELIVERY INSPECTION - - UNDER VEHICLE - 14. SUSPENSION SYSTEM | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation