[54A] CHASSIS ELECTRICAL - - HEADLAMP - ON-VEHICLE SERVICE - BULB REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| BULB REPLACEMENT
| <2000>
| Headlamp bulb <low-beam> CAUTION Do not touch the bulb surface bare-handed or with dirty gloves. If dirt is attached on surface of the bulb, immediately use alcohol or thinner to remove dirt, and install the bulb after well dried. Disconnect the headlamp connector.
| Screw out the headlamp socket. Replace the valve, and connect securely the connector.
| Headlamp bulb <high-beam> CAUTION Do not touch the bulb surface bare-handed or with dirty gloves. If dirt is attached on surface of the bulb, immediately use alcohol or thinner to remove dirt, and install the bulb after well dried. Disconnect the headlamp connector.
| Twist the socket to withdraw the bulb. Replace the valve, and connect securely the connector.
| Position lamp bulb CAUTION Do not touch the bulb surface bare-handed or with dirty gloves. If dirt is attached on surface of the bulb, immediately use alcohol or thinner to remove dirt, and install the bulb after well dried.
| Disconnect the connector, and twist the position lamp socket to remove it.
| <2400>
| Headlamp bulb (low beam)
| CAUTION Do not touch the surface of the bulb with hands or dirty gloves as the bulb may pop after a short time. If the surface does become dirty, clean it with alcohol or thinner, and let it dry thoroughly before installing. Disconnect the connector. Remove the socket cover.
| Release the bulb securing spring, and remove the bulb. Replace the valve, and connect the connector securely.
| Headlamp bulb (high beam)
| CAUTION Do not touch the surface of the bulb with hands or dirty gloves as the bulb may pop after a short time. If the surface does become dirty, clean it with alcohol or thinner, and let it dry thoroughly before installing. Disconnect the connector. Twist the socket to withdraw the bulb. Replace the valve, and connect the connector securely.
| Position lamp bulb CAUTION Do not touch the bulb surface bare-handed or with dirty gloves. If dirt is attached on surface of the bulb, immediately use alcohol or thinner to remove dirt, and install the bulb after well dried.
| Twist the socket to withdraw the bulb. Replace the valve, and connect the connector securely.
| Front turn-signal lamp bulb CAUTION Do not touch the bulb surface bare-handed or with dirty gloves. If dirt is attached on surface of the bulb, immediately use alcohol or thinner to remove dirt, and install the bulb after well dried.
| Twist the socket to withdraw the bulb. Replace the valve, and connect the connector securely.

[54A] CHASSIS ELECTRICAL - - HEADLAMP - ON-VEHICLE SERVICE - BULB REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation