[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - SIDE IMPACT SENSOR - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION WARNING If any problems, replace the sensor. Check the side impact sensor and bracket for dents, cracks or deformation. Check the connector for damage, and terminal for deformation. Check that there is no bending or corrosion in the centre pillar. NOTE: For the checks other than the items above, refer to Troubleshooting (Refer to ) .

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - SIDE IMPACT SENSOR - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation