[14] ENGINE COOLING - - WATER HOSE AND WATER PIPE - REMOVAL AND INSTALLATION <4G6-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G6-DOHC>
Pre-removal and Post-installation Operation Engine Coolant Draining and Supplying (Refer to .) Intercooler Removal and Installation (Refer to GROUP 15, Intercooler .) Air Cleaner Removal and Installation (Refer to GROUP 15, Air Cleaner .) Thermostat Removal and Installation (Refer to .)
|  |  | Removal steps
--- | --- | --- | ---
<<A>> | >>C<< | 1. | Radiator upper hose connection
| >>B<< | 2. | Water outlet fitting
|  | 3. | Vacuum hose
|  | 4. | Engine hanger
|  | 5. | Solenoid valve assembly
|  | 6. | Water hose
|  | 7. | Water hose
|  | 8. | Water hose
|  | 9. | Turbocharger water feed pipe
|  | 10. | Gasket
| >>B<< | 11. | Thermostat case assembly
|  | 12. | Water hose
|  | • | Turbocharger assembly (Refer to GROUP 15, Exhaust manifold and turbocharger assembly .)
|  | 13. | Turbocharger water return pipe
|  | 14. | Gasket
|  | 15. | Heater hose connection
|  | 16. | Water inlet pipe assembly
| >>A<< | 17. | O-ring
| REMOVAL SERVICE POINT
| <<A>> RADIATOR UPPER HOSE DISCONNECTION
| After making mating marks on the radiator hose and hose clamp, disconnect the radiator hose.
| INSTALLATION SERVICE POINTS
| >>A<< O-RING INSTALLATION
| CAUTION Do not allow engine oil or other grease to adhere to the O-ring Insert the O-ring to the water pipe, and coat the outer portion of the O-ring with water or engine coolant.
| >>B<< THERMOSTAT CASE ASSEMBLY/WATER OUTLET FITTING INSTALLATION Use a gasket scraper or wire brush to completely eliminate all gasket material on the gasket mounting surface. Apply a bead of the specified sealant. Specified Sealant: MITSUBISHI GENUINE PART No. MD970389 or equivalent With the sealant still wet (within 15 minutes after the sealant is applied), install the thermostat case or water outlet fitting. Do not apply the sealant in an area more than the required.
| >>C<< RADIATOR UPPER HOSE CONNECTION
| Insert each hose as far as the projection of the water outlet fitting. Align the mating marks on the radiator hose and hose clamp, and then connect the radiator hose.

[14] ENGINE COOLING - - WATER HOSE AND WATER PIPE - REMOVAL AND INSTALLATION <4G6-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation