[54B] SMART WIRING SYSTEM (SWS) - - ADJUSTMENT FUNCTION <VEHICLES FOR HONG KONG SPEC.> | PRINT PAGE / INDEX / PRIOR / NEXT

ADJUSTMENT FUNCTION <VEHICLES FOR HONG KONG SPEC.>
<WHEN MUT-II/III AND SWS MONITOR IS NOT USED> The security alarm can be enabled/disabled and the plenary alarm time can be changed in accordance with the adjustment mode entry conditions by operating the switches. The programmed information is held even when the battery is disconnected.
ENTRY CONDITIONS OF THE ADJUSTING MODE Set switches to the following conditions: Driver's door switch ON (The driver’s door is open.) Key reminder switch: ON (Remove the ignition key.) Lighting switch: OFF Turning ON the windshield washer switch for 10 seconds or more (pull the wiper lever toward you) sounds the ETACS-ECU build-in buzzer, and the adjusting mode is entered. With keeping this state (keeping on pulling the wiper lever toward you), each pressing of the unlock switch on the transmitter switches the settings.
ADJUSTING THE SECURITY ALARM FUNCTION The security alarm function will be enabled/disabled and plenary alarm time will be changed in the sequence below. (After "c", it goes back to "a" repeating in alphabetical order.) Security alarm function is disabled. (the initial condition): Tone alarm sounds once. Security alarm function is enabled. (Warning: hazard and horn): The buzzer sounds three times. Security alarm function is enabled. (Warning: hazard only): The buzzer sounds five times.
RELEASE CONDITIONS FOR THE ADJUSTMENT MODE The adjustment mode will be cancelled under one of the following conditions: Driver's door switch OFF (The driver's door is closed.) Key reminder switch: OFF (Insert the ignition key.) Lighting switch: ON Windshield washer switch: OFF When 30 seconds have elapsed without pressing the unlock switch of the keyless entry transmitter NOTE: In order to enter the adjustment mode, the wiper/washer switch and the transmitter must be operated. However, the wipers/washers or the keyless entry system will not work at this time. This adjustment function is also described in the Owners Handbook so that customers can use it.
<WHEN MUT-II/III AND SWS MONITOR ARE USED> Using MUT-II/III adjusts the following function. The programmed information is held even when the battery is disconnected. Door-ajar warning function Driving with any door, including a tailgate, not properly closed sounds the buzzer, and blinks the door-ajar indicator lamp on the combination meter to let the driver know the door-ajar state. Turn signal lamp operation tone function Synchronized with the hazard lamp and the turn signal lamp, the buzzer sounds. Hazard answer back function of the keyless entry system When lock/unlock is operated with the keyless entry transmitter, the hazard lamp blinks, so that the driver can check the vehicle lock/unlock state being near by it. Power window and sunroof operation of multimode keyless entry system From near by vehicle, the driver can actuate power window and the sunroof by operating the keyless entry transmitter. Timer lock time after executing the keyless entry unlock If any door including a tailgate is not opened after being unlocked with the keyless transmitter, doors are locked automatically within the specified time. Timer function time of power window and sunroof Even after turning OFF (LOCK) the ignition switch, the power window and the sunroof can be operated for the specified time. Power window lock operation on the driver's seat Pressing the power window lock switch build-in the power window main switch enables the power window operation by the power window main switch except for the driver's seat. Vehicle speed-dependent wiper function With the windshield wiper switch in the intermittent position, the intermittent duration changes depending on the intermittent adjusting knob position and the vehicle speed. Rear wiper intermittent duration When the rear wiper switch is turned ON, the rear wiper operates in the intermittent action. In addition, when the rear wiper switch is operated continuously, the rear wiper works continuously. Electric folding door mirror automatic unfolding function Driving with the door mirror retracted resets the door mirror automatically. Using other methods to retract/reset the door mirror is available. Auto lamp function sensor sensitivity (illumination intensity) When the lighting switch is in the AUTO position, the position lamp and headlamp illuminate automatically depending on the ambient brightness level. Headlamp automatic shutdown function When the ignition switch is turned OFF (LOCK) while the lighting switch is in the TAIL, AUTO or HEAD position, and then the driver's door is opened, the heap lamp is turned off automatically for preventing the unattended operation. The delay-off time of the room lamp When the door is closed with the ignition switch OFF (LOCK), the interior lamp is turned off automatically in the specified time. Interior lamp automatic shutdown function If the interior lamp such as the room lamp is kept on with the ignition switch OFF (LOCK), the lamp is turned off automatically after the specified time. Security alarm Operative/inoperative state of the security alarm function is selected. Action adjustment during the power window key off timer operation Operating the power window other than the driver's seat is available during the power window timer operation. Initializing all functions (Returning to the initial condition) All adjusting functions are returned to the settings at the time of factory shipment.
Item No. | Item (MUT-II/III display) | Item | Adjusting contents (MUT-II/III display) | Adjusting contents
--- | --- | --- | --- | ---
1 | PHOTO SENSOR | Auto lamp function sensor sensitivity (illumination intensity) | HIGH ILLUMIN | High ambient brightness
STD ILLUMIN | Standard ambient brightness (initial setting)
LOW ILLUMIN | Low ambient brightness
LO LO ILLUMIN | Low-low ambient brightness
2 | H/L AUTO-CUT | Headlamp automatic shutdown function | W.FUNCTION(A) | With function: The automatic tail lamp turn off function with the ignition switch OFF (LOCK) is available.
W.FUNCTION(D) | With function: The automatic tail lamp turn off with the ignition switch OFF (LOCK) is not available. (the initial condition)
W/O FUNCTION | Without function
4 | SPEED SEN WIP | Vehicle speed-dependent wiper function | W.FUNCTION | With function (the initial condition)
W/O FUNCTION | Without function
5 | WING MIRROR | Electric folding door mirror automatic unfolding function | SPEED SEN FUN | Vehicle speed sensing reset (the initial condition)
IG-LINKED FUN | Ignition linked
KEYLESS LINK | Keyless entry linked
W/O FUNCTION | Without function
9 | KEYLESS(HAZD) | Hazard answer back function of the keyless entry system | LOCK/UNLOCK | With function for lock/unlock (the initial condition)
LOCKED | With function only for lock
UNLOCKED | Without function only for unlock
W/O FUNCTION | Without function
10 | KEYLESS(P/W) | Power window and sunroof operation of multimode keyless entry system | OPEN/CLOSE | With function of close and open actions (the open action is for the power window only.)
CLOSE | With function the close action only (the initial condition)
W/O FUNCTION | Without activation
11 | SECURITY ALM | Security alarm | HORN/HAZARD | With function: hazard and horn):
HAZARD | With function: hazard only):
W/O FUNCTION | Without function (the initial condition)
15 | T/SIG.BUZZER | Turn signal lamp operation tone function | W.FUNCTION | With function
W/O FUNCTION | Without function (the initial condition)
16 | RM LMP TN OFF | The delay-off time of the room lamp | 60s | 60 seconds
30s | 30 seconds
15s | 15 seconds (the initial condition)
7.5s | 7.5 seconds
W/O FUNCTION | 0 second (no delay action)
18 | KEY-OFF TMR T | Power window· sunroof timer functioning duration | W/O FUNCTION | Without the timer function
30s | 30 seconds (the initial condition)
3min. | 3 minutes
10min. | 10 minutes
19 | P/W KEY OFF T | Action adjustment during the power window key off timer operation * | NORMAL ACTION | Accepting the normal operation during the timer operation (the initial condition)
M S/W RESTRC. | Operating the power windows (except for the driver's seat) by the power window main switch is prohibited during the timer operation.
24 | KEYLES LOCK T | Timer lock time after executing the keyless entry unlock | 30s | 30 seconds (the initial condition)
60s | 1 minutes
120s | 2 minutes
180s | 3 minutes
26 | DOOR WARN BUZ | Door-ajar warning function | W.FUNCTION | With function (the initial condition)
W/O FUNCTION | Without function
27 | WIPR-LINK H/L | Wiper-linked auto lamp function | W/O FUNCTION | Without function (the initial condition)
ONLY A/LP OPE | With function
28 | R.INT WIPER T | Rear wiper intermittent duration | 8s | 8 seconds: Without continuous operation (the initial condition)
4s(W SUCSSON) | 4 seconds: With continuous operation
8s(W SUCSSON) | 8 seconds: With continuous operation
16s(W SUCSSO) | 16 seconds: With continuous operation
CONTIN ACTION | Continuous operation (without the intermittence)
30 | RM/L AUTO-CUT | Interior lamp automatic shutdown function | 3min. | With auto-turn off: 3 minutes
30min. | With auto-turn off: 30 minutes (the initial condition)
60min. | With auto-turn off: 60 minutes
W/O FUNCTION | Without auto-turn off
31 | P/W LOCK MODE | Power window lock operation on the driver's seat | ALL SEATS OPE | Operating all seats is available when lock is ON. (the initial condition)
ONLY DR SEAT | Operating seats other than the driver's seat is prohibited when lock is ON.
NOTE: * : For details, refer to the workshop manual.

[54B] SMART WIRING SYSTEM (SWS) - - ADJUSTMENT FUNCTION <VEHICLES FOR HONG KONG SPEC.> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation