[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - ON-VEHICLE SERVICE - SPEEDOMETER CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| ON-VEHICLE SERVICE

| SPEEDOMETER CHECK
| Adjust the pressure of tires to the specified level. (Refer to GROUP 31, On-vehicle Service ). CAUTION Do not operate the clutch suddenly. Do not increase/decrease speed rapidly while testing.
| CAUTION Set a free-roller on the rear tyre for 4WD.
| Set the vehicle onto a speedometer tester and use wheel chocks to hold the rear wheels.
| To prevent the front wheel from moving from side to side, attach tension bars to the tie-down hook, and secure both ends to anchor plates. To prevent the vehicle from moving, attach a chain or wire to the rear retraction hook, and make sure the end of the chain or wire is secured. Check if the speedometer indicator range is within the standard values. Standard value:
Vehicles for 180 km/h speedometer
Standard indicator km/h | Allowance range km/h
--- | ---
20 | 17 -23
40 | 38 - 43
80 | 79 - 84
120 | 120 - 125
160 | 161 - 166
Vehicles for 130 MPH speedometer
Standard indicator MPH | Allowance range MPH
--- | ---
10 | 10 -13
25 | 25 - 28
50 | 50 - 54
75 | 76 - 80
100 | 102 - 106
125 | 127 - 132
Vehicles for 220 km/h speedometer <Except for Australia and New zealand (2400)>
Standard indicator km/h | Allowance range km/h
--- | ---
20 | 20 - 24
40 | 40 - 44
80 | 80 - 86
120 | 122 - 128
160 | 163 - 170
200 | 204 - 212
Vehicles for Australia and New zealand (2400)
Standard indicator km/h | Allowance range km/h
--- | ---
20 | 18 - 22
40 | 38 - 42
80 | 79 - 84
120 | 120 - 125
160 | 161 - 166
200 | 202 - 207
| If not to the standard value, inspect for proper tyre size. If not correct, replace the tires with original size tyres and retest. If correct, replace the speedometer. If still not to standard value, replace the vehicle speed sensor.

[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - ON-VEHICLE SERVICE - SPEEDOMETER CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation