[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Items | Specifications
--- | ---
Basic idle speed r/min | 700 ± 50 <SOHC> 700 ± 50 <DOHC>
Throttle position sensor adjusting voltage mV | 535 - 735
Throttle position sensor resistance kΩ | 3.5 - 6.5
Idle speed control servo coil resistance (at 20°C) Ω | 28 - 33
Intake air temperature sensor resistance kΩ | -20°C | 13 - 17
0°C | 5.3 - 6.7
20°C | 2.3 - 3.0
40°C | 1.0 - 1.5
60°C | 0.56 - 0.76
80°C | 0.30 - 0.42
Engine coolant temperature sensor resistance kΩ | -20°C | 14 - 17
0°C | 5.1 - 6.5
20°C | 2.1 - 2.7
40°C | 0.9 - 1.3
60°C | 0.48 - 0.68
80°C | 0.26 - 0.36
Oxygen sensor output voltage (at racing) V <SOHC> | 0.6 - 1.0
Oxygen sensor heater resistance (at 20°C) Ω<SOHC> | Front | 4.5 - 8.0
Rear | 11 - 18
Oxygen sensor heater resistance (at 20°C) Ω <DOHC> | 4.5 - 8.0
Injector coil resistance (at 20°C) Ω | 13 - 16
Fuel pressure control solenoid valve resistance (at 20°C) Ω <DOHC> | 28 - 36

[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation