[11B] ENGINE OVERHAUL <4G6-SOHC> - - REWORK DIMENSIONS | PRINT PAGE / INDEX / PRIOR / NEXT

REWORK DIMENSIONS
Items | Standard value
--- | ---
CYLINDER HEAD AND VALVES
Diameter of oversize valve seat ring hole in cylinder head mm | Intake | 0.03 oversize | 34.30 - 34.33
0.06 oversize | 34.60 - 34.63
Exhaust | 0.03 oversize | 31.80 - 31.83
0.06 oversize | 32.10 - 34.13
Diameter of oversize valve guide hole in cylinder head mm | 0.05 oversize | 11.05 - 11.07
0.25 oversize | 11.25 - 11.27
0.50 oversize | 11.50 - 11.52

[11B] ENGINE OVERHAUL <4G6-SOHC> - - REWORK DIMENSIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation