[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - INSPECTION PROCEDURE A-2: Communication with the column switch (column-ECU) is not possible. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE A-2: Communication with the column switch (column-ECU) is not possible.
| CAUTION Whenever the ECU is replaced, ensure that the power supply circuit, the grounding circuit and the communication circuit are normal.
| COMMENTS ON TROUBLE SYMPTOM The power supply circuit to the column switch (column-ECU) may be defective. If the wiring harness of the battery power supply circuit for the ECU (column switch terminal No.1) is defective, also check the power supply circuit to the ignition switch (IG1) (column switch terminal No.9) and repair if necessary.
| TROUBLESHOOTING HINTS Malfunction of the ETACS-ECU Malfunction of the column switch Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. ECU check by using the SWS monitor Check that the power supply and earth lines to the ETACS-ECU and the SWS communication lines are normal. Ignition switch: ON ECU TO BE CHECKED ETACS ECU OK: "OK" is displayed on the "ETACS ECU" menu. Q: Is the check result normal? YES: Go to Step 2. NO: Refer to Inspection Procedure A-3 "Communication with ETACS-ECU is not possible ."
| Step 2. Connector check: C-310 column switch connector Q: Is the check result normal? YES: Go to Step 3. NO: Repair the defective connector.
| Step 3. Measure the voltage at C-310 column switch connector. Disconnect the connector, and measure at the connector side. Voltage between C-310 column switch connector No.1 and body earth OK: Battery positive voltage Q: Is the check result normal? YES: Go to Step 5. NO: Go to Step 4.
| Step 4. Check the wiring harness between C-310 column switch connector terminal No.1 and fusible link (1). NOTE: Prior to the wiring harness inspection, check intermediate connector A-14 <RH drive vehicle>, C-116 <LH drive vehicle>, C-125 <RH drive vehicle>, junction block connector C-204, C-202, joint connectors C-02 <LH drive vehicle>, and repair if necessary. Check the power supply line for open circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 5. Measure the resistance at C-310 column switch connector. Disconnect the connector, and measure at the connector side. Continuity between C-310 column switch connector No.4 and body earth OK: 2 Ω or less Q: Is the check result normal? YES: Go to Step 7. NO: Go to Step 6.
| Step 6. Check the wiring harness between C-310 column switch connector No.4 and body earth Check the earth wires for open circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 7. Connector check: C-219 ETACS-ECU connector Q: Is the check result normal? YES: Go to Step 8. NO: Repair the defective connector.
| Step 8. Check the wiring harness from C-219 ETACS-ECU connector terminal Nos.59 and 68 to C-310 column switch connector terminal Nos.3 and 2. NOTE: Prior to the wiring harness inspection, check joint connector C-02, and repair if necessary. Check the communication lines for open circuit. Q: Is the check result normal? YES: Go to Step 9. NO: Repair the wiring harness.
| Step 9. ECU check by using the SWS monitor Ignition switch: ON ECU TO BE CHECKED COLUMN ECU OK: "OK" is displayed on the "COLUMN ECU" menu. Q: Is the check result normal? YES: Go to Step 10. NO: Replace the column switch.
| Step 10. Retest the system. Check that the ETACS-ECU communicates with the column switch. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the ETACS-ECU.

[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - INSPECTION PROCEDURE A-2: Communication with the column switch (column-ECU) is not possible. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation