[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - TROUBLESHOOTING - INSPECTION CHART FOR DIAGNOSIS CODE | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION CHART FOR DIAGNOSIS CODE Follow the inspection chart that is appropriate for the diagnosis code.
Diagnosis code No. | Inspection item | Diagnostic content | Reference page
--- | --- | --- | ---
11 | Front right ABS sensor | Open circuit or short circuit |
12 | Front left ABS sensor
13 | Rear right ABS sensor
14 | Rear left ABS sensor
16 | Power supply system | ABS-ECU power supply voltage below or above the standard value. Not displayed if the voltage recovers. |
21 | Front right ABS sensor |
22 | Front left ABS sensor
23 | Rear right ABS sensor
24 | Rear left ABS sensor
32 | G sensor system <4WD> |
33 | Stoplight switch system |
41 | ABS front right solenoid valve |
42 | ABS front left solenoid valve
43 | ABS rear right solenoid valve
44 | ABS rear left solenoid valve
51 | Valve relay problem (stays on) | Replace the hydraulic unit (Integrated with ABS-ECU).
52 | Valve relay problem (stays off) or ABS-ECU power supply system problem |
53 | Motor relay problem (stays off) or ABS-ECU power supply system problem
54 | Motor relay problem (stays on) | Replace the hydraulic unit (Integrated with ABS-ECU).
55 | Motor system (seized pump motor) or ABS-ECU power supply system problem |
63 | ABS-ECU | Replace the hydraulic unit (Integrated with ABS-ECU).
NOTE: diagnosis code No.16, 52, 63 Code No. 16 is cleared from the memory by turning the ignition switch to ACC position. When the system is properly reset, this code is also cleared from the memory. Code No. 52 and 63 are cleared from the memory by turning the ignition switch to ACC position.

[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - TROUBLESHOOTING - INSPECTION CHART FOR DIAGNOSIS CODE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation