[14] ENGINE COOLING - - RADIATOR - REMOVAL AND INSTALLATION <4G63-SOHC, 4G64-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

RADIATOR

REMOVAL AND INSTALLATION <4G63-SOHC, 4G64-SOHC>
Pre-removal Operation Engine Coolant Draining (Refer to ). Air Cleaner Removal (Refer to GROUP 15, Air Cleaner ). | Post-installation Operation Air Cleaner Installation (Refer to GROUP 15, Air Cleaner ). Engine Coolant Refilling and Level Check (Refer to ).
|  |  | Radiator removal steps
--- | --- | --- | ---
|  | 1. | Drain plug
|  | 2. | O-ring
|  | 3. | Radiator cap
|  | 4. | Radiator condenser tank hose
|  | 5. | Radiator condenser tank assembly
|  | 6. | Cooling fan controller connector
<<A>> | >>A<< | 7. | Radiator upper hose
<<A>> | >>A<< | 8. | Radiator lower hose
<<B>> |  | 9. | A/T fluid cooler hose connection
|  | 10. | Upper insulator
|  | 11. | Radiator assembly
|  | 12. | Lower insulator
|  | 13. | A/T fluid cooler hose assembly
|  | 14. | Cooling fan controller
|  | 15. | Cooling fan motor & shroud assembly
|  |  | Cooling fan motor removal steps
|  | 4. | Radiator condenser tank hose
|  | 6. | Cooling fan controller connector
<<A>> | >>A<< | 7. | Radiator upper hose
|  | 15. | Cooling fan assembly
|  | 16. | Cooling fan
|  | 17. | Cooling fan motor
|  | 18. | Cooling fan shroud
| REMOVAL SERVICE POINTS
| <<A>> RADIATOR UPPER HOSE/RADIATOR LOWER HOSE DISCONNECTION
| Make mating marks on the radiator hose and the hose clamp. Disconnect the radiator hose.
| <<B>> A/T FLUID COOLER HOSE DISCONNECTION After disconnecting the hose, plug it to avoid entry of dust or foreign material.
| INSTALLATION SERVICE POINT
| >>A<< RADIATOR LOWER HOSE/RADIATOR UPPER HOSE CONNECTION
| Insert each hose as far as the projection of the water inlet fitting. Align the mating marks on the radiator hose and hose clamp, and then connect the radiator hose.

[14] ENGINE COOLING - - RADIATOR - REMOVAL AND INSTALLATION <4G63-SOHC, 4G64-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation