[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - TROUBLESHOOTING - HOW TO CONNECT THE SWS MONITOR | PRINT PAGE / INDEX / PRIOR / NEXT

| HOW TO CONNECT THE SWS MONITOR CAUTION Always turn the ignition switch to the "LOCK" (OFF) position before connecting or disconnecting the SWS monitor and the MUT-II/III.
| HOW TO CONNECT THE SWS COMMUNICATION LINE <SWS MONITOR HARNESS (FOR COLUMN-ECU)>
| Remove the steering column cover. Remove the steering column switch connector. Connect the SWS monitor harness (for column-ECU).
| HOW TO CONNECT THE SWS COMMUNICATION LINE <SWS MONITOR HARNESS (FOR 13-PIN CONNECTOR)>
| Connect the SWS monitor harness (for 13-pin connector) to the diagnosis connector (13-pin connector).

[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - TROUBLESHOOTING - HOW TO CONNECT THE SWS MONITOR | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation