[16] ENGINE ELECTRICAL - - STARTING SYSTEM - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Item | Standard value | Limit
--- | --- | ---
Pinion gap mm | 0.5 - 2.0 | -
Commutator run-out mm | 0.05 | 0.1
Commutator diameter mm | 29.4 | 28.8
Undercut depth mm | 0.5 | 0.2

[16] ENGINE ELECTRICAL - - STARTING SYSTEM - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation