[37] POWER STEERING - - ON-VEHICLE SERVICE - TIE ROD END BALL JOINT DUST COVER CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| TIE ROD END BALL JOINT DUST COVER CHECK Press the dust cover with your finger to check whether the dust cover is cracked or damaged. If the dust cover is cracked or damaged, replace the tie rod end. NOTE: If the dust cover is cracked or damaged, the ball joint could be damaged.

[37] POWER STEERING - - ON-VEHICLE SERVICE - TIE ROD END BALL JOINT DUST COVER CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation