[15] INTAKE AND EXHAUST - - EXHAUST MANIFOLD AND TURBOCHARGER - TURBOCHARGER ASSEMBLY DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

TURBOCHARGER ASSEMBLY DISASSEMBLY AND REASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Snap ring
|  | 2. | Waste gate actuator
|  | 3. | Coupling
| >>D<< | 4. | Turbine housing
<<A>> | >>C<< | 5. | Snap ring
<<B>> | >>B<< | 6. | Cartridge assembly
|  | 7. | Compressor cover
| >>A<< | 8. | O-ring
| DISASSEMBLY SERVICE POINTS
| <<A>> SNAP RING REMOVAL
| CAUTION Hold the snap ring with your fingers during its removal to prevent it from springing away. Remove the compressor cover retaining snap ring using a snap ring pliers.
| <<B>> CARTRIDGE ASSEMBLY REMOVAL
| CAUTION The cartridge assembly may be stuck on the compressor cover by the O-ring. Loosen the cartridge assembly before removal by lightly tapping the compressor cover all around with a plastic hammer.
| CLEANING Use a clean washing solvent available on the market to wash the turbocharger components. Use a plastic scraper or bristle brush for cleaning aluminum parts.
| REASSEMBLY SERVICE POINTS
| >>A<< O-RING INSTALLATION
| CAUTION Be careful not to damage the O-ring during installation. Damaged O-ring could cause leaks. Smear engine oil on the inside surface of a new O-ring and fit it in the groove of the cartridge assembly.
| >>B<< CARTRIDGE ASSEMBLY INSTALLATION Smear engine oil on the inside of the O-ring fitted on the cartridge assembly.
| CAUTION Be careful not to damage the vanes of the cartridge assembly when installing the cartridge assembly onto the compressor cover. Install the cartridge assembly onto the compressor cover, aligning the dowel pin with its hole.
| >>C<< SNAP RING INSTALLATION
| CAUTION Install the snap ring with its chamfer facing up. Place the set of cartridge assembly and compressor cover upright on the compressor cover and install the snap ring in position.
| >>D<< TURBINE HOUSING INSTALLATION
| CAUTION Be careful not to damage the vanes of the cartridge assembly when installing the turbine housing. Pay attention to alignment of the turbine housing. Assemble the set of compressor cover and cartridge assembly with the turbine housing while aligning the dowel pin with its hole.

[15] INTAKE AND EXHAUST - - EXHAUST MANIFOLD AND TURBOCHARGER - TURBOCHARGER ASSEMBLY DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation