[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Items | Specifications
--- | ---
Intake air temperature sensor resistance kΩ | -20°C | 13 - 17
0°C | 5.3 - 6.7
20°C | 2.3 - 3.0
40°C | 1.0 - 1.5
60°C | 0.56 - 0.76
80°C | 0.30 - 0.42
Engine coolant temperature sensor resistance kΩ | -20°C | 14 - 17
0°C | 5.1 - 6.5
20°C | 2.1 - 2.7
40°C | 0.9 - 1.3
60°C | 0.48 - 0.68
80°C | 0.26 - 0.36
Oxygen sensor output voltage (at racing) V | 0.6 - 1.0
Oxygen sensor heater resistance (at 20°C) Ω | front | 11 - 18 <Vehicles except for Brazil, Chile and Hong kong> 4.5 - 8.5 <Vehicles for Brazil, Chile and Hong kong>
rear | 11 - 18 <Vehicles for Brazil and Chile> 4.5 - 8.5 <Vehicles for Hong kong>
Fuel pressure kPa | Approximately. 324 at curb idle
Injector coil resistance (at 20°C) Ω | 10.5 - 13.5
Throttle valve control servo coil resistance (at 20°C) Ω | 0.3 - 80
Oil control valve (at 20°C) Ω | 6.9 - 7.9

[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation