[00E] GENERAL <ELECTRICAL> - - HOW TO READ WIRING DIAGRAMS - WIRE COLOUR CODE | PRINT PAGE / INDEX / PRIOR / NEXT

WIRE COLOUR CODE
| Wire colours are identified by the following colour codes.
Code | Wire colour | Code | Wire colour | Code | Wire colour | Code | Wire colour
--- | --- | --- | --- | --- | --- | --- | ---
B | Black | L | Blue | R | Red | Y | Yellow
BR | Brown | LG | Light green | SB | Sky blue | - | -
G | Green | O | Orange | V | Violet | - | -
GR | Grey | P | Pink | W | White | - | -
| If a cable has two colours, the first of the two colour code characters indicates the basic colour (colour of the cable coating) and the second indicates the marking colour.
No. | Meaning
--- | ---
1 | <F>: Flexible wire
<T>: Twisted wire
2 | Wire size (mm2 )*
3 | Basic colour (colour of the cable coating)
4 | Marking colour
NOTE: *: No code indicates 0.5 mm2 . Cable colour code in parentheses indicates 0.3 mm2 .

[00E] GENERAL <ELECTRICAL> - - HOW TO READ WIRING DIAGRAMS - WIRE COLOUR CODE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation