[1] PRE-DELIVERY INSPECTION - - AFTER ROAD TEST - 35. RADIATOR COOLANT LEVEL | PRINT PAGE / INDEX / PRIOR / NEXT

| 35. RADIATOR COOLANT LEVEL
| Check that the coolant level in the reserve tank is at or above "LOW" mark at normal engine operating temperature. And check cooling system for leaks. Check that the coolant concentration is 30% to 60%. CAUTION Do not remove the radiator cap while the cooling system is under pressure. When removing the radiator cap, be careful of steam and boiling water. Add coolant only to the reserve tank if it is required.

[1] PRE-DELIVERY INSPECTION - - AFTER ROAD TEST - 35. RADIATOR COOLANT LEVEL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation