[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 20: Sound Quality is Poor, or Sound is Weak. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 20: Sound Quality is Poor, or Sound is Weak.
DIAGNOSIS PROCEDURE
STEP 1. Check that the player works normally if the tape is changed. NOTE: Check that the tape label is not loose, that the tape case is not deformed and that the tape is tightly wound. Also, tapes with a length of C-120 or greater can often get caught in the mechanism and should not be used. Q: Does the player work normally if the tape is changed? YES: The tape used is defective. NO: Go to Step 2.
STEP 2. Check that the player play OK if the tape player head is cleaned. Q: Does the player play OK if the tape player head is cleaned? YES: The sound quality should return to normal. NO: Go to Step 3.
STEP 3. Check that the proper operation is obtained when the tape player is replaced. Q: Is proper operation obtained when the tape player is replaced? YES: Replace the radio and tape player. The sound quality should return to normal. NO: Repair or replace the speakers. The sound quality should return to normal.

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 20: Sound Quality is Poor, or Sound is Weak. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation