[4] CORROSION PROTECTION - - ROCKER PANEL PRIMER APPLICATION LOCATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

ROCKER PANEL PRIMER APPLICATION LOCATIONS
To prevent rusting from chipping (flying rock), a priming panel primer has been applied to the areas indicated in the figure. The priming panel primer is applied between the under and middle coat. It improves anti-corrosive performance by preventing flying rock to damage the body panel with the primer application, according to the thickness and elasticity of the primer. Apply the primer before the middle coat when replacing the panel complete with a priming panel primer application.

[4] CORROSION PROTECTION - - ROCKER PANEL PRIMER APPLICATION LOCATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation