[42] BODY - - TAILGATE - TAILGATE HANDLE AND LATCH - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

TAILGATE HANDLE AND LATCH

REMOVAL AND INSTALLATION
Post-installation Operation Tailgate Handle Play Check (Refer to ).
|  |  | Striker removal steps
--- | --- | --- | ---
|  | ·• | Rear end trim (Refer to GROUP 52A, Trims .)
| >>A<< | 1. | Striker
|  |  | Tailgate lock key cylinder removal steps
|  | • | Tailgate lower trim (Refer to GROUP 52A, Tailgate Trim .)
|  | 2. | Tailgate lock key cylinder
|  |  | Tailgate handle removal steps
|  | • | Tailgate lower trim (Refer to GROUP 52A, Tailgate Trim .)
|  | 3. | Tailgate handle
|  |  | Tailgate latch assembly removal steps
|  | • | Tailgate lower trim (Refer to GROUP 52A, Tailgate Trim .)
|  | 4. | Earth bolt
|  | 5. | Tailgate latch assembly
|  |  | Tailgate lock actuator removal steps
|  | • | Tailgate lower trim (Refer to GROUP 52A, Tailgate Trim .)
|  | 6. | Tailgate lock actuator
| INSTALLATION SERVICE POINT
| >>A<< STRIKER INSTALLATION
| Assemble so the distance between the centre of the striker and centre of the latch is ±1.5 mm or less.

[42] BODY - - TAILGATE - TAILGATE HANDLE AND LATCH - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation