[54A] CHASSIS ELECTRICAL - - REAR WINDOW DEFOGGER - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

REAR WINDOW DEFOGGER

| GENERAL INFORMATION
| Rear Defogger operation The defogger relay turns ON if the defogger switch built-in the A/C-ECU is turned ON when the ignition switch is in the "ON" position. When the defogger relay turns ON, power is supplied to the defogger and the defogger is activated. The defogger comes with a timer function that causes the defogger switch to automatically turn OFF in about 11 minutes after the defogger switch is turned ON.

[54A] CHASSIS ELECTRICAL - - REAR WINDOW DEFOGGER - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation