[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - THROTTLE BODY ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

THROTTLE BODY ASSEMBLY

REMOVAL AND INSTALLATION
CAUTION Do not loosen the fixing screws for the resin cover of throttle body assembly. If the screws are loosened, the sensor incorporated in the resin cover becomes misaligned and the throttle body can not work normally.
Pre-removal Operation Engine Coolant Draining (Refer to GROUP 14, On-vehicle Service - Engine Coolant Replacement ). Air Cleaner Removal (Refer to GROUP 15, Air Cleaner ). | Post-installation Operation Air Cleaner Installation (Refer to GROUP 15, Air Cleaner ). Engine Coolant Supplying (Refer to GROUP 14, On-vehicle Service - Engine Coolant Replacement ).
|  |  | Removal steps
--- | --- | --- | ---
| >>B<< | • | Initialisation procedure (installation only)
|  | 1. | Throttle position sensor connector
|  | 2. | Water return hose connection
|  | 3. | Water feed hose connection
|  | 4. | Throttle body assembly
| >>A<< | 5. | Throttle body gasket
| INSTALLATION SERVICE POINT
| >>A<< THROTTLE BODY GASKET INSTALLATION CAUTION Poor idling etc. may result if the throttle body gasket is installed incorrectly.
| Install the throttle body gasket as its protrusion is in the direction shown.
| >>B<< INITIALISATION PROCEDURE Turn the ignition switch on then off, and keep it off for at least 10 seconds.

[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - THROTTLE BODY ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation