[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS UNDER THE VEHICLE - B11. CHANGE GEAR OIL IN FRONT AND REAR DIFFERENTIAL | PRINT PAGE / INDEX / PRIOR / NEXT

| B11. CHANGE GEAR OIL IN FRONT AND REAR DIFFERENTIAL Remove the drain plug to discharge the gear oil. Fit the drain plug and tighten it to the specified torque. Tightening torque: 64 ± 4 N·m
| Remove the filler plug and add the specified gear oil up to the bottom end of the filler plug hole. Specified gear oil: Gear oil API classification GL-5 or higher Above 10°C SAE 90 Below 10°C SAE 80W Quantity: 0.55 L Fit the filler plug and tighten it to the specified torque. Tightening torque: 49 ± 9 N·m

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS UNDER THE VEHICLE - B11. CHANGE GEAR OIL IN FRONT AND REAR DIFFERENTIAL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation