[42] BODY - - DOOR - ON-VEHICLE SERVICE - CENTRAL DOOR LOCKING SYSTEM INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| CENTRAL DOOR LOCKING SYSTEM INSPECTION Check the system as described below. If the system does not work, carry out troubleshooting. Refer to GROUP 54B, Troubleshooting , refer to GROUP 54C, Troubleshooting , refer to GROUP 54D, Troubleshooting or refer to GROUP 54E, Troubleshooting . Check that the central door locking system works by operating the driver's door key cylinder, the passenger’s door key cylinder <Except vehicles for Hong Kong spec> and the driver’s door inside lock knob. NOTE: When the inside lock knob is operated with the driver's door opened, the driver's door is not locked. Check whether the driver's door is opened when the driver's door inside handle is pulled with all the doors locked. Also check whether all the doors (including the tailgate) are unlocked simultaneously.

[42] BODY - - DOOR - ON-VEHICLE SERVICE - CENTRAL DOOR LOCKING SYSTEM INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation