[27B] REAR AXLE <4WD> - - DIFFERENTIAL CARRIER ASSEMBLY - DIFFERENTIAL SUPPORT MEMBER BUSHING REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| DIFFERENTIAL SUPPORT MEMBER BUSHING REPLACEMENT
| <DIFFERENTIAL MOUNT BRACKET>
| Use special tool rear suspension bushing arbor (MB990883) to remove or install the bushing. Press-fit the bushing with its hollow portion facing in the direction shown. Press-fit the bushing until the bushing outer case end face is flush with the differential mount bracket.
| <DIFFERENTIAL SUPPORT ARM>
| Use special tool mount bushing arbor (MB990984) to remove or install the bushing. Press-fit the bushing with its marks facing in the direction shown. Press-fit the bushing until the bushing outer case end face is flush with the differential support arm.

[27B] REAR AXLE <4WD> - - DIFFERENTIAL CARRIER ASSEMBLY - DIFFERENTIAL SUPPORT MEMBER BUSHING REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation