[54A] CHASSIS ELECTRICAL - - REAR WINDOW DEFOGGER - REAR WINDOW DEFOGGER SWITCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| DEFOGGER RELAY CHECK
Battery voltage | Tester connection | Specified condition
--- | --- | ---
Not supplied | 4 - 5 | Open circuit
Connect terminal 1 to the positive battery terminal Connect terminal 3 to the negative battery terminal | 4 - 5 | Less than 2 ohms

[54A] CHASSIS ELECTRICAL - - REAR WINDOW DEFOGGER - REAR WINDOW DEFOGGER SWITCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation