[14] ENGINE COOLING - - THERMOSTAT - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| THERMOSTAT CHECK
| Immerse the thermostat in water, and heat the water while stirring. Check the thermostat valve opening temperature. Standard value: 82 ± 1.5°C
| Check that the amount of valve lift is at the standard value when the water is at the full-opening temperature. NOTE: Measure the valve height when the thermostat is fully closed, and use this measurement to compare the valve height when the thermostat is fully open. Standard value: Full-opening temperature: 95°C Amount of valve lift: 8.5 mm or more

[14] ENGINE COOLING - - THERMOSTAT - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation