[15] INTAKE AND EXHAUST - - AIR CLEANER - REMOVAL AND INSTALLATION <4G63-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G63-DOHC>
CAUTION Parts marked by * are made of recycled-paper mixed plastic material, so observe the following precautions. Avoid any shock or load to these parts when removing and installing them. When installing, securely set the air cleaner body assembly clamp to the air cleaner cover. NOTE: Parts marked by * are made of recycled-paper mixed plastic material. Dispose of according to state and local laws
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Air duct
|  | 2. | Air cleaner cover
|  | 3. | Air cleaner element
|  | 4. | Air flow sensor connector
|  | 5. | Air cleaner body and air flow sensor assembly
|  | 6. | Air flow sensor assembly
|  | 7. | Gasket
|  | 8. | Air cleaner body assembly
|  | • | Air by-pass valve and intercooler outlet air hose B assembly
|  | 9. | Breather hose connection
|  | 10. | Vacuum hose connection
|  | 11. | Air intake hose
|  | 12. | Air cleaner bracket

[15] INTAKE AND EXHAUST - - AIR CLEANER - REMOVAL AND INSTALLATION <4G63-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation