[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - SUNROOF - INSPECTION PROCEDURE F-4: Sunroof anti-trap function does not work normally. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE F-4: Sunroof anti-trap function does not work normally.
| CAUTION Whenever the ECU is replaced, ensure that the input and output signal circuits are normal.
| COMMENTS ON TROUBLE SYMPTOM If the sunroof anti-trap function does not work, the sunroof motor assembly (sunroof-ECU) may be defective.
| POSSIBLE CAUSES Malfunction of the sunroof motor assembly (sunroof-ECU)
| DIAGNOSIS PROCEDURE
| Retest the system. Check that the sunroof anti-trap function work normally. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the sunroof motor assembly.

[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - SUNROOF - INSPECTION PROCEDURE F-4: Sunroof anti-trap function does not work normally. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation