[15] INTAKE AND EXHAUST - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Item | Standard value | Limit
--- | --- | ---
Turbocharger supercharging pressure (waste gate solenoid valve not operating) kPa | 59 - 84 | -
Initial activation pressure of waste gate actuator (at the stroke of approximately 1 mm) kPa | Approximately 80 | -
Waste gate solenoid valve coil resistance (at 20°C) Ω | 29 - 35 | -
Initial activation pressure of air bypass valve kPa | Approximately 53 | -
Manifold distortion of the installation surface mm | 0.15 or less | 0.20

[15] INTAKE AND EXHAUST - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation