[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G64-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - DIAGNOSTIC TROUBLE CODE PROCEDURES - Code No.16 Auto-cruise Control-ECU System | PRINT PAGE / INDEX / PRIOR / NEXT

Code No.16 Auto-cruise Control-ECU System
DIAGNOSIS CODE SET CONDITIONS This diagnosis code is set if there is an abnormality in the cancel hold circuit or the microprocessor monitor circuit in the auto-cruise control-ECU.
PROBABLE CAUSE Malfunction of the auto-cruise control-ECU.
DIAGNOSIS Replace the auto-cruise control-ECU (Refer to ). Then check that MUT-II/III diagnosis code No. 16 is not set.

[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G64-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - DIAGNOSTIC TROUBLE CODE PROCEDURES - Code No.16 Auto-cruise Control-ECU System | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation