[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

SPECIAL TOOLS
Tool | Number | Name | Use
--- | --- | --- | ---
| MB990784 | Ornament remover | Removal of instrument panel driver’s side garnish and meter bezel.
| MB991502 | MUT-II sub assembly | Reading MPI system diagnosis code
| MB991955 A: MB991824 B: MB991827 C: MB991910 D: MB991911 E: MB991825 F: MB991826 | MUT-III sub-assembly A: Vehicle Communication Interface (V. C. I.) B: MUT-III USB cable C: MUT-III main harness A (Vehicles with CAN communication system) D: MUT-III main harness B (Vehicles without CAN communication system) E: MUT-III measurement adapter F: MUT-III trigger harness | Reading MPI system diagnosis code CAUTION MUT-III main harness B (MB991911) should be used. MUT-III main harness A should not be used for this vehicle.
| MB991223 A: MB991219 B: MB991220 C: MB991221 D: MB991222 | Harness set A: Test harness B: LED harness C: LED harness adapter D: Probe | Making voltage and resistance measurements during troubleshooting A: Connect pin contact pressure inspection B: Power circuit inspection C: Power circuit inspection D: Commercial tester connection

[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation