[27B] REAR AXLE <4WD> - - DIFFERENTIAL CARRIER ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

DIFFERENTIAL CARRIER ASSEMBLY

REMOVAL AND INSTALLATION
Pre-removal Operation Main Muffler and Centre Exhaust Pipe Removal (Refer to GROUP 15, Exhaust Pipe and Muffler.) Differential Gear Oil Draining Drive Shaft Removal (Refer to .) | Post-installation Operation Drive Shaft Installation (Refer to .) Differential Gear Oil Filling (Refer to.) Main Muffler and Centre Exhaust Pipe Installation (Refer to GROUP 15, Exhaust Pipe and Muffler.) Rear Wheel Alignment Check and Adjustment (Refer to GROUP 34, On-vehicle Service-Rear Wheel Alignment Check and Adjustment.)
|  |  | Removal steps
--- | --- | --- | ---
<<A>> | >>B<< | 1. | Propeller shaft connection
|  | 2. | Self-locking nut
|  | 3. | Dynamic damper
|  | 4. | Differential support arm connecting bolt
|  | 5. | Self-locking nut
|  | 6. | Differential support member bolt
|  | 7. | Lower stopper
|  | 8. | Upper stopper
|  | 9. | Differential support member
|  | 10. | Gasket
|  | 11. | Packing
|  | 12. | Differential mount bracket
|  | 13. | Differential carrier assembly
|  | 14. | Rear suspension crossmember
|  | 15. | Differential support arm
|  |  | Removal steps
--- | --- | --- | ---
<<A>> | >>B<< | 1. | Propeller shaft connection
|  | 2. | Self-locking nut
|  | 3. | Dynamic damper
|  | 4. | Differential support arm connecting bolt
|  | 5. | Self-locking nut
|  | 6. | Rear differential support weight
|  | 7. | Differential support arm
| >>A<< | 8. | Breather hose assembly
|  | 9. | Differential mount bracket bolt
|  | 10. | Weight
|  | 11. | Lower stopper
|  | 12. | Upper stopper
|  | 13. | Differential mount bracket
|  | 14. | Gasket
|  | 15. | Packing
|  | 16. | Differential carrier assembly
| REMOVAL SERVICE POINT
| <<A>> PROPELLER SHAFT DISCONNECTION
| Make mating marks on the differential companion flange and the propeller shaft assembly. Suspend the removed propeller shaft from the body with a wire to prevent bending.
| INSTALLATION SERVICE POINTS
| >>A<< BREATHER HOSE ASSEMBLY INSTALLATION CAUTION Be careful not to apply grease, water or soapy water to the hose inlet.
| Fully insert the breather hose into the vent plug. Install the breather hose pad as shown in the illustration.
| >>B<< PROPELLER SHAFT INSTALLATION Align the mating marks of differential companion flange and propeller shaft assembly.

[27B] REAR AXLE <4WD> - - DIFFERENTIAL CARRIER ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation