[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - CENTRAL DOOR LOCKING SYSTEM - INSPECTION PROCEDURE C-5: The impact detection door unlock function does not function. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE C-5: The impact detection door unlock function does not function.
| CAUTION Whenever the ECU is replaced, ensure that the input and output signal circuits are normal.
| COMMENTS ON TROUBLE SYMPTOM If the impact detection door unlock function does not work normally, the input signal circuit from the impact detection sensor, the SRS-ECU or the ETACS-ECU may be defective.
| POSSIBLE CAUSES Malfunction of the SRS-ECU Malfunction of the ETACS-ECU Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Use the MUT-II/III to confirm a diagnosis code. (MUT-II/III diagnosis code) Check whether the ETACS-ECU sets diagnosis code No.31 or 32. Q: Is the diagnosis code set? YES: Refer to . NO: Replace the ETACS-ECU.

[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - CENTRAL DOOR LOCKING SYSTEM - INSPECTION PROCEDURE C-5: The impact detection door unlock function does not function. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation