[8] REFERENCE MATERIAL - - INSTALLATION AND REMOVAL OF ADHESIVE COMPONENTS - SIDE SILL GARNISH | PRINT PAGE / INDEX / PRIOR / NEXT

INSTALLATION AND REMOVAL OF ADHESIVE COMPONENTS

SIDE SILL GARNISH
<20V, R, GLX, LS>
<SPORT GEAR, GLS, XLS, LTD>
| REMOVAL
| SIDE SILL GARNISH REMOVAL Gently lift and remove the side sill garnish. If there is any double-sided tape remaining on the side sill garnish, remove according to the following instructions. <Remove double-side tape remaining on the body surface>
| Attach protection tape all the way along the edges of the double-sided tape which is still adhering to the body.
| Scrape off the double-sided tape with a resin spatula as possible. Peel off the protection tape. Wipe the body surface and clean it with a rag moistened with isopropyl alcohol.
| <Remove double-sided tape remaining on side sill garnish and adhere double-sided tape (when re-using side sill garnish)>
| Scrape off the double-sided tape on the side sill garnish with a resin spatula as possible. Wipe the side sill garnish surface and clean it with a rag moistened with isopropyl alcohol. Remove only a small portion of the residual adhesive. Adhere the double-sided tape as specified on the side sill garnish.
| INSTALLATION
| SIDE SILL GARNISH INSTALLATION
| Tear off the double-sided tape backing paper. NOTE: If you attach the adhesive tape to the edge of the backing paper, it will be easy to tear off. Install the side sill garnish. NOTE: If the double-sided tape is difficult to affix in cold temperature, etc., warm the bonding surfaces of the body and side sill garnish to about 40 - 60°C before affixing the tape. Firmly press in the side sill garnish.
| PROTECT FILM INSTALLATION <SPORT GEAR, GLS, XLS, LTD> Installation position CAUTION
| The ambient temperature should be 20 to 38°C. Ensure that the working area is clean. If ambient temperature is less than 20°C, heat the protect film and application surface to a temperature of 20 to 30°C. Be careful that air bubbles are not formed under the protect film. Installation procedure Wipe the protect film application surface and clean it with a rag moistened with isopropyl alcohol. Remove backing paper from the protect film, and apply the film to the specified position.

[8] REFERENCE MATERIAL - - INSTALLATION AND REMOVAL OF ADHESIVE COMPONENTS - SIDE SILL GARNISH | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation