[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR

SERVICE SPECIFICATIONS
Item | Standard value
--- | ---
Speedometer indication | Vehicles for 180 km/h speedometer | 20 | 17 - 23
40 | 38 - 43
80 | 79 - 84
120 | 120 - 125
160 | 161 - 166
Vehicles for 130 MPH speedometer | 10 | 10 - 13
25 | 25 - 28
50 | 50 - 54
75 | 76 - 80
100 | 102 - 106
125 | 127 - 132
Vehicles for 220 km/h speedometer <Except for Australia and New zealand> | 20 | 20 - 24
40 | 40 - 44
80 | 80 - 86
120 | 122 - 128
160 | 163 - 170
200 | 204 - 212
Vehicles for Australia and New zealand | 20 | 18 - 22
40 | 38 - 42
80 | 79 - 84
120 | 120 - 125
160 | 161 - 166
200 | 202 - 207
Tachometer indication error r/min | 700 | 700 ± 100
2,000 | 2,000 ± 100
3,000 | 3,000 ± 150
4,000 | 4,000 ± 200
5,000 | 5,000 ± 250
6,250 | 6,250 ± 150
Fuel gauge unit resistance Ω | Fuel pump and gauge unit | Float position F (highest) | 1.5 ± 0.5
Float position E (lowest) | 55 ± 1.5
Fuel gauge unit | Float position F (highest) | 1.5 ± 0.5
Float position E (lowest) | 55 ± 1.5
Fuel gauge unit float height mm | Fuel pump and gauge unit | Float position F (At) | 36.7 ± 2
Float position E (B) | 149.6 ± 2
Fuel gauge unit | Float position F (A) | 23.4 ± 2
Float position E (B) | 194.2 ± 2
Engine coolant temperature gauge unit resistance Ω | 104 + 13.5 (at 70°C)

[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation