[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 25: Tape gets Caught in Mechanism. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 25: Tape gets Caught in Mechanism. NOTE: When the tape is caught in the mechanism, the tape case may not eject. When this occurs, do not try to force the tape out as this may damage the tape player mechanism. Take the cassette to a service dealer for repair.
DIAGNOSIS PROCEDURE
STEP 1. Check that the player works normally if tape is changed. NOTE: Check that the tape label is not loose, that the tape itself is not deformed and that the tape is tightly wound. Also, tape with a length of C-120 or greater can often get caught in the mechanism and should not be used. Q: Does the player work normally if tape is changed? YES: The tape used is defective. The tape player should operate normally. NO: Replace the radio and tape player. The procedure is complete.

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 25: Tape gets Caught in Mechanism. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation