[11C] ENGINE MECHANICAL <4G6-DOHC> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION
Item | 4G63
--- | ---
Total displacement mL | 1,997
Bore × Stroke mm | 85 × 88
Compression ratio | 9.0
Compression chamber | Pentroof
Camshaft arrangement | DOHC
Number of valve | Intake | 8
Exhaust | 8
Valve timing | Intake opening | BTDC 17°
Intake closing | ABDC 51°
Exhaust opening | BBDC 57°
Exhaust closing | ATDC 13°
Fuel system | Electronically controlled multipoint fuel injection
Rocker arm | Roller type
Auto-lash adjuster | Equipped

[11C] ENGINE MECHANICAL <4G6-DOHC> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation