[54A] CHASSIS ELECTRICAL - - HAZARD WARNING LAMP SWITCH - TROUBLESHOOTING | PRINT PAGE / INDEX / PRIOR / NEXT

TROUBLESHOOTING
FLASHER TIMER FUNCTION The hazard warning lamps (flasher timer function) are controlled by the Smart Wiring System (SWS). For troubleshooting, refer to respective Groups below. Not using SWS monitor <Hong Kong spec.>: GROUP 54B, Troubleshooting . Using SWS monitor <Hong Kong spec.>: GROUP 54C, Troubleshooting . Not using SWS monitor <Except for Hong Kong spec.>: GROUP 54D, Troubleshooting . Using SWS monitor <Except for Hong Kong spec.>: GROUP 54E, Troubleshooting .

[54A] CHASSIS ELECTRICAL - - HAZARD WARNING LAMP SWITCH - TROUBLESHOOTING | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation