[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - EVAPORATIVE EMISSION CONTROL SYSTEM - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| EVAPORATIVE EMISSION VENTILATION SOLENOID CHECK
| Connect a hand vacuum pump to nipple (A) of the solenoid. Check air tightness by applying a vacuum with voltage applied directly from the battery to the evaporative emission ventilation solenoid and without applying voltage.
Battery Voltage | Normal Condition
--- | ---
Applied | Vacuum maintained
Not applied | Vacuum leaks
| Measure the resistance between the terminals of the solenoid. Standard value: 17 - 21 Ω (at 20°C)

[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - EVAPORATIVE EMISSION CONTROL SYSTEM - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation