[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A19. REPLACE FUEL FILTER | PRINT PAGE / INDEX / PRIOR / NEXT

| A19. REPLACE FUEL FILTER Remove the rear seat cushion assembly.
| Remove the service hole cover.
| Disconnect the harness connector, fuel hose and fuel tube. Unscrew the mounting nuts to remove the fuel pump module.
| Remove the fuel filter from fuel pump module. Install the new fuel filter. CAUTION Apply a unleaded petrol to the grommet and O-ring before installing them in order to prevent damage.
| Install the fuel pump module. Tighten the mounting nuts to the specified torque. Specified torque: 2.5 ± 0.4 N·m
| Connect the fuel hose, fuel tube and harness connector.
| CAUTION After connecting the fuel high-pressure hose or fuel pump suction tube <4WD>, slightly pull it to ensure that it is installed securely. Also confirm that there is a play approximately 3mm. Install the service hole cover. Install the rear seat cushion assembly.

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A19. REPLACE FUEL FILTER | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation