[42] BODY - - DOOR - ON-VEHICLE SERVICE - CIRCUIT BREAKER (INCORPORATED IN THE POWER WINDOW MOTOR) INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| CIRCUIT BREAKER (INCORPORATED IN THE POWER WINDOW MOTOR) INSPECTION
| Pull the power window switch to the UP position to fully close the door window glass, and keep pulling the switch for 10 additional seconds. Release the power window switch from the UP position and immediately press it to the DOWN position. The condition of the circuit breaker is good if the door window glass starts to move downwards within 60 seconds.

[42] BODY - - DOOR - ON-VEHICLE SERVICE - CIRCUIT BREAKER (INCORPORATED IN THE POWER WINDOW MOTOR) INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation